; Windows Modem Setup File
; Copyright (c) 1993-1995 Microsoft Corporation
; Manufacturer: Rockwell
; Supports Rockwell & some Cirrus chipset modems, encompassing many mfgs & models

[Version]
Signature="$CHICAGO$"
Class=Modem
Provider=%Rockwell%

[ControlFlags]
ExcludeFromSelect=UNIMODEM733C4E29                   ; Zoom, Best Data, 28.8 internal combo
ExcludeFromSelect=UNIMODEMA3EEEF33                   ; Zoom, Best Data, 28.8 external combo
ExcludeFromSelect=UNIMODEM24FFB24B                   ; CPI, Best Data 9648Fx External
ExcludeFromSelect=UNIMODEM1058B7F8                   ; V.34 Apex, Toshiba
ExcludeFromSelect=UNIMODEMCFA485CD,UNIMODEM2C9A8C70  ; 14000 bps Data-Fax internal
ExcludeFromSelect=UNIMODEMC9720A17                   ; Logicode, Microcom
ExcludeFromSelect=UNIMODEMAF48CC9F                   ; Premax, Smart Modular 
ExcludeFromSelect=UNIMODEM526F22F6                   ; Piiceon PCMCIA 14.4 and 14.4 for Contura+LTE (ISA)
ExcludeFromSelect=UNIMODEMCC96FDC7                   ; Cardinal v.34 and CPI (Viva)
ExcludeFromSelect=UNIMODEM1C445CDD                   ; Cardinal v.34 and CPI (Viva)
ExcludeFromSelect=UNIMODEMAAC52F50                   ; Cardinal MVP144IF, MVP144E
ExcludeFromSelect=PCMCIA\PIICEON-DISPATCHER-80D0     ; Piiceon Dispatcher V.34, 14.4
ExcludeFromSelect=UNIMODEME466C599                   ; Reveal, Packard Bell

[Manufacturer]
%Rockwell%   = Rockwell
%Cardinal%   = Cardinal
%Digitan%    = Digitan
%BestData%   = BestData   
%SMART%      = SMART   
%Apex%       = Apex
%ComOne%     = ComOne
%Logicode%   = Logicode
%Premax%     = Premax
%Macronix%   = Macronix
%Piiceon%    = Piiceon
%Mitsubishi% = Mitsubishi
%Winbook%    = Winbook
%Reveal%     = Reveal

[Reveal]
%Reveal1%  = Rockwell20, UNIMODEM8CF33BE4   ; Reveal V.34, 28.8, internal
%Reveal2%  = Rockwell10, ROCK_Reveal2, UNIMODEM535147EF   ; Reveal 14.4, Data FAX, internal
%Reveal4%  = Rockwell44, ROCK_Reveal4, UNIMODEME466C599   ; Reveal 14.4 Modem Soundcard
%Reveal5%  = Rockwell44, UNIMODEME466C599   ; Reveal, Packard Bell

[Winbook]
%Winbook1% = Rockwell31, UNIMODEM0BCCA4A7    ; WinbookXP 14.4 internal modem
%Winbook2% = Rockwell43, ROCK_Winbook2, UNIMODEM858E1599    ; WinbookXP cirrus chipset

[Mitsubishi]
%Mitsubishi1% = Rockwell14, PCMCIA\MITSUBISHI_ELECTRIC_CORPORATION-MF0B-004____________-2B0E ; Mitsubishi 14.4 PCMCIA
%Mitsubishi1% = Rockwell14, UNIMODEM0715F8AD                                                 ; Mitsubishi 14.4 PCMCIA

[Piiceon]
%Piiceon2% = Rockwell29, PCMCIA\PIICEON-DISPATCHER-3CDB  ; Piiceon Dispatcher 14.4 PCMCIA
%Piiceon2% = Rockwell29, PCMCIA\PIICEON-DISPATCHER-3A96  ; Piiceon Dispatcher 14.4 PCMCIA
%Piiceon2% = Rockwell29, ROCK_Piiceon2, UNIMODEM526F22F6                ; Piiceon Dispatcher 14.4 PCMCIA
%Piiceon2% = Rockwell29, ROCK_Piiceon2, PCMCIA\PIICEON-DISPATCHER-80D0  ; Piiceon Dispatcher 14.4 PCMCIA
%Piiceon3% = Rockwell30, UNIMODEMA4A014C2                ; Piiceon Dispatcher V.34 
%Piiceon4% = Rockwell33, ROCK_Piiceon4, UNIMODEM526F22F6                ; Piiceon Dispatcher 14.4 for LTE and Contura
%Piiceon5% = Rockwell33, UNIMODEM526F22F6                ; combo, Piiceon PCMCIA 14.4 and 14.4 for Contura+LTE (ISA)
%Piiceon6% = Rockwell34, UNIMODEME8277FDB                ; Piiceon Dispatcher 14.4 for Toshiba
%Piiceon7% = Rockwell40, ROCK_Piiceon7, PCMCIA\PIICEON-DISPATCHER-80D0  ; Piiceon Dispatcher V.34 PCMCIA
%Piiceon7% = Rockwell40, ROCK_Piiceon7, UNIMODEMAF48CC9F                ; Piiceon Dispatcher V.34 PCMCIA
%Piiceon8% = Rockwell29, PCMCIA\PIICEON-DISPATCHER-80D0  ; Piiceon Dispatcher V.34, 14.4 PCMCIA

[Macronix]
%Macronix1% = Rockwell14, PCMCIA\MACRONIX-FAX/MODEM-B6E7   ; Macronix 14.4 PCMCIA
%Macronix1% = Rockwell14, UNIMODEM8EA167E0                 ; Macronix 14.4 PCMCIA
%Macronix2% = Rockwell28, UNIMODEM22C3B64D                 ; Macronix 1200 ISA

[Premax]
%Premax1% = Rockwell13, PCMCIA\PREMAX-FM288_-92E2     ; Premax 28.8, V.34 PCMCIA
%Premax1% = Rockwell13, ROCK_Premax1, UNIMODEMAF48CC9F              ; Premax 28.8, V.34 PCMCIA
%Premax2% = Rockwell13, PCMCIA\PREMAX-FM288I-DC97     ; Premax 28.8, VFC PCMCIA
%Premax2% = Rockwell13, UNIMODEM90FBBB54              ; Premax 28.8, VFC PCMCIA
%Premax3% = Rockwell41, UNIMODEMAF48CC9F              ; combo, premax, Smart Modular, Piiceon

[Logicode]
%Logicode1% = Rockwell19, UNIMODEM5F5D689E      ; Logicode 28.8 V.34 External with cell
%Logicode2% = Rockwell20, ROCK_Logicode2, UNIMODEM1C445CDD      ; Logicode 28.8 V.34 Internal with cell
%Logicode3% = Rockwell21, ROCK_Logicode3, UNIMODEMCFA485CD      ; Logicode 14.4 Internal data-fax-voice with cell
%Logicode4% = Rockwell22, ROCK_Logicode4, UNIMODEMC9720A17      ; Logicode 14.4 External data-fax-voice with cell
%Logicode5% = Rockwell23, UNIMODEMC9720A17      ; Logicode and Microcom combo
%Logicode6% = Rockwell22, UNIMODEMF48FCB61      ; Logicode 14.4 External data-fax 
%Logicode7% = Rockwell24, ROCK_Logicode7, UNIMODEM16E3BF9F      ; Logicode 14.4 Internal data-fax
%Logicode8% = Rockwell25, UNIMODEM9A52F7F4      ; Logicode 9624 Internal data-fax
%Logicode9% = Rockwell26, UNIMODEM6C57C7DE      ; Logicode 9624 External data-fax
%Logicode13% = Rockwell10, ROCK_Logicode13, UNIMODEM535147EF    ; Logicode 14.4 RPI style

[Rockwell]
%Rockwell1% = Rockwell1, UNIMODEM959C40CA       ; 14000 bps Data-Fax internal
%Rockwell2% = Rockwell2, UNIMODEMCFA485CD       ; 14000 bps Data-Fax internal
%Rockwell3% = Rockwell18,UNIMODEM2C9A8C70       ; 14000 bps Data-Fax internal

[Cardinal]
%Cardinal1% = Rockwell1,   ROCK_Cardinal1, UNIMODEM959C40CA      ; Shipped by Zeos
%Cardinal2% = Rockwell19,  ROCK_Cardinal2, UNIMODEMCC96FDC7      ; Cardinal 28.8, V.34 external
%Cardinal3% = Rockwell35,  UNIMODEMCC96FDC7      ; Cardinal 28.8, V.34 external, CPI (Viva)
%Cardinal4% = Rockwell36,  UNIMODEMCE29838A      ; Cardinal 14.4 mvp144xf
%Cardinal5% = Rockwell37,  ROCK_Cardinal5, UNIMODEMAAC52F50      ; Cardinal 14.4 mvp144e
%Cardinal6% = Rockwell12,  ROCK_Cardinal6, UNIMODEM24FFB24B      ; Cardinal 14.4 mvp24xf
%Cardinal7% = Rockwell14,  PCMCIA\CARDINAL-MVP144PCMCIA-5538     ; Cardinal 14.4 PCMCIA, MVP144PCMCIA
%Cardinal7% = Rockwell14,  ROCK_Cardinal7, UNIMODEMD3A140D7      ; Cardinal 14.4 PCMCIA, MVP144PCMCIA
%Cardinal8% = Rockwell20,  ROCK_Cardinal8, UNIMODEM1C445CDD      ; Cardinal 28.8, V.34, internal MVP288I
%Cardinal9% = Rockwell38,  UNIMODEM1C445CDD      ; Cardinal 28.8, V.34, internal MVP288I
%Cardinal10% = Rockwell39, ROCK_Cardinal10, UNIMODEMAAC52F50     ; Cardinal 14.4 Data FAX MVP144IF
%Cardinal11% = Rockwell37, UNIMODEMAAC52F50      ; Cardinal 14.4 Data FAX MVP144IF
%Cardinal12% = Rockwell10, ROCK_Cardinal12, UNIMODEM16A162D5     ; Cardinal 14.4 Data FAX MVP144I
%Cardinal13% = Rockwell11, ROCK_Cardinal13, UNIMODEM9F2BBC58     ; Cardinal 2400 Data FAX MB2650SR
%Cardinal14% = Rockwell42, UNIMODEMFFB2F7FF      ; Cardinal 19.2 data fax MVP192I

[Digitan]
%Digitan2%  = Rockwell2,  ROCK_Digitan2, UNIMODEMCFA485CD      ; Shipped by Dell
%Digitan3%  = Rockwell20, ROCK_Digitan3, UNIMODEMEAF8FBCB      ; Digitan V.34 with voice
%Digitan4%  = Rockwell20, ROCK_Digitan4, UNIMODEM733C4E29      ; Digitan V.34

[BestData]
%BestData1%  = Rockwell3, UNIMODEM4643BBB7      ; Best Data 1442FX External 
%BestData2%  = Rockwell4, UNIMODEM96F16EB5      ; Best Data 1442F Internal
%BestData3%  = Rockwell5, ROCK_BestData3, UNIMODEM733C4E29      ; Best Data 2834F Internal
%BestData4%  = Rockwell6, UNIMODEM733C4E29      ; Best Data 2834F Internal and Zoom V.34 internal combo
%BestData5%  = Rockwell7, ROCK_BestData5, UNIMODEMA3EEEF33      ; Best Data 2834FX External 
%BestData6%  = Rockwell8, UNIMODEMA3EEEF33      ; Best Data 2834FX External and Zoom V.34 internal combo
%BestData7%  = Rockwell9, ROCK_BestData7, UNIMODEM798B889B      ; Best Data 1442FX External (FTX, RPI model)
%BestData8%  = Rockwell10, ROCK_BestData8, UNIMODEM535147EF     ; Best Data 1442FX Internal (FT, RPI model)
%BestData8%  = Rockwell10, UNIMODEM145054C5     ; Best Data 1442FX Internal (FT, RPI model)
%BestData9%  = Rockwell11, ROCK_BestData9, UNIMODEM9F2BBC58     ; Best Data 9624FQ Internal
%BestData10%  = Rockwell11, UNIMODEM65278A40    ; Best Data 2400B Internal
%BestData11%  = Rockwell12, UNIMODEMDC7EB890    ; Best Data 9648FX External
%BestData11%  = Rockwell12, ROCK_BestData11, UNIMODEM24FFB24B    ; Best Data 9648FX External
%BestData12%  = Rockwell12, UNIMODEM24FFB24B    ; Best Data 9648FX External and viva combo
%BestData13%  = Rockwell12, ROCK_BestData13, UNIMODEM24FFB24B    ; Best Data 2400X External

[SMART]
%SmartMod1%  = Rockwell14, UNIMODEMDE96F803                      ; Smart ST1414 PCMCIA
%SmartMod1%  = Rockwell14, PCMCIA\INTELLIGENT-FAXMODEM-F938      ; Smart ST1414 PCMCIA
%SmartMod2%  = Rockwell13, ROCK_SmartMod2, UNIMODEMAF48CC9F      ; Smart V.34 PCMCIA
%SmartMod2%  = Rockwell13, PCMCIA\SMART_MODULAR_ST2814-E3BD      ; Smart V.34 PCMCIA

[Apex]
%Apex3% = Rockwell15, ROCK_Apex3, PCMCIA\RIPICAA-RC144ACL-845A      ; Apex V.34
%Apex3% = Rockwell15, PCMCIA\AD_PC_CARD-RC288ACL-5DA6   ; Apex V.34
%Apex3% = Rockwell15, ROCK_Apex3, UNIMODEM1058B7F8                  ; Apex V.34
%Apex4% = Rockwell15, UNIMODEM1058B7F8                  ; Apex V.34 and Toshiba combo

[ComOne]
%ComOne6% = Rockwell13, PCMCIA\COM1_SA-MC218_CARD-415E                ; MC218 28.8 PCMCIA
%ComOne6% = Rockwell13, UNIMODEM7A03E29F                              ; MC218 28.8 PCMCIA
%ComOne4% = Rockwell17, ROCK_ComOne4, PCMCIA\AT&T_PARADYNE-KEEPINTOUCH_CARD-762F    ; MC216
%ComOne2% = Rockwell16, PCMCIA\COM1_SA-MC214_CARD-5738                ; MC214A 
%ComOne2% = Rockwell16, UNIMODEMD3A0F28F                              ; MC214A
%ComOne1% = Rockwell14, PCMCIA\COM1_SA-MC217_CARD-15FC                ; MC217A 14.4 PCMCIA
; ComOne tuples from untested/unavailable models
; %ComOne13% = Rockwell-n, PCMCIA\PHILIPS-S214_CARD_-D9F4
; %ComOne12% = Rockwell-n, PCMCIA\TOSHIBA-_SLIMFAXII-F6F4
; %ComOne11% = Rockwell-n, PCMCIA\PHILIPS-S218_CARD_-DBDE
; %ComOne10% = Rockwell-n, PCMCIA\TOSHIBA-SLIMV34___-B57C
; %ComOne9% = Rockwell-n, PCMCIA\PHILIPS-S217_CARD_-7791
; %ComOne8% = Rockwell-n, PCMCIA\CXR_SA_-AJ_1448___-E24C
; %ComOne7% = Rockwell-n, PCMCIA\TOSHIBA-SLIM144___-7781
; %ComOne5% = Rockwell20                                             ;external
; %ComOne3% = Rockwell18                                             ;external              

; Installation sections

[Rockwell1] ; (internal/external 14400)
AddReg=All, MfgAddReg, Rockwell1.AddReg, EXTERNAL

[Rockwell2] ; (internal 14400)
AddReg=All, MfgAddReg, Rockwell2.AddReg, INTERNAL

[Rockwell3] ; (external 14400) - Best Data
AddReg=All, MfgAddReg, Rockwell3.AddReg, EXTERNAL

[Rockwell4] ; (internal 14400) - Best Data
AddReg=All, MfgAddReg, Rockwell4.AddReg, INTERNAL

[Rockwell5] ; (internal 28.8) - Best Data
AddReg=All, MfgAddReg, Rockwell5.AddReg, INTERNAL

[Rockwell6] ; (internal 28.8) - Best Data and Zoom combo
AddReg=All, MfgAddReg, Rockwell6.AddReg, INTERNAL

[Rockwell7] ; (external 28.8) - Best Data
AddReg=All, MfgAddReg, Rockwell5.AddReg, EXTERNAL

[Rockwell8] ; (external 28.8) - Best Data and zoom combo
AddReg=All, MfgAddReg, Rockwell6.AddReg, EXTERNAL

[Rockwell9] ; (external 14400) - Best Data 1442FX (FTX, RPI model)
AddReg=All, MfgAddReg, Rockwell9.AddReg, EXTERNAL

[Rockwell10] ; (internal 14400) - Best Data 1442FX (FT, RPI model)
AddReg=All, MfgAddReg, Rockwell10.AddReg, INTERNAL

[Rockwell11] ; (internal 2400) - Best Data 9624FQ 
AddReg=All, MfgAddReg, Rockwell11.AddReg, INTERNAL

[Rockwell12] ; (external 2400) - Best Data 9648Fx, 2400B, 2400X and other modems
AddReg=All, MfgAddReg, Rockwell12.AddReg, EXTERNAL  

[Rockwell13] ; Smart V.34 PCMCIA
AddReg=All, MfgAddReg, Rockwell13.AddReg, PCMCIA 

[Rockwell14] ; SMART ST1414 PCMCIA with cell
AddReg=All, MfgAddReg, Rockwell14.AddReg, PCMCIA 

[Rockwell15] ; Apex V.34 PCMCIA and Tosh combo. 
AddReg=All, MfgAddReg, Rockwell15.AddReg, PCMCIA 

[Rockwell16] ; PCMCIA 2400 bps, 19.2 max dte, no cell
AddReg=All, MfgAddReg, Rockwell16.AddReg, PCMCIA 

[Rockwell17] ; Com1 by AT&T-KeepinTouch PCMCIA
AddReg=All, MfgAddReg, Rockwell17.AddReg, PCMCIA

[Rockwell18] ; (internal 14400) - no speed negotiation, inactivity timer is \Tn with max 90 minutes
AddReg=All, MfgAddReg, Rockwell18.AddReg, INTERNAL

[Rockwell19] ; V.34 external with cell
AddReg=All, MfgAddReg, Rockwell13.AddReg, EXTERNAL

[Rockwell20] ; V.34 internal with cell
AddReg=All, MfgAddReg, Rockwell13.AddReg, INTERNAL

[Rockwell21] ; (internal 14400) - with cell
AddReg=All, MfgAddReg, Rockwell21.AddReg, INTERNAL

[Rockwell22] ; (external 14400) - Logicode data-fax-voice with cell
AddReg=All, MfgAddReg, Rockwell22.AddReg, EXTERNAL

[Rockwell23] ; (external 14400)  Logicode and Microcom combo
AddReg=All, MfgAddReg, Rockwell23.AddReg, EXTERNAL

[Rockwell24] ; (internal 14400) - cirrus chipset found in Logicode, no cell
AddReg=All, MfgAddReg, Rockwell24.AddReg, INTERNAL

[Rockwell25] ; (internal 2400) - Logicode 9426
AddReg=All, MfgAddReg, Rockwell25.AddReg, INTERNAL

[Rockwell26] ; (external 2400) - Logicode 9426
AddReg=All, MfgAddReg, Rockwell25.AddReg, EXTERNAL

[Rockwell28] ; (internal 1200)  - no compr, ec, speed neg, hard flow, cell
AddReg=All, MfgAddReg, Rockwell28.AddReg, INTERNAL

[Rockwell29] ; Piiceon Dispatcher 14.4 with cell
AddReg=All, MfgAddReg, Rockwell29.AddReg, PCMCIA 

[Rockwell30] ; Piiceon Dispatcher V.34
AddReg=All, MfgAddReg, Rockwell30.AddReg, INTERNAL

[Rockwell31] ; Winbook 14.4 Internal
AddReg=All, MfgAddReg, Rockwell31.AddReg, INTERNAL

[Rockwell33] ; internal 14.4 Dispatcher *OR* combo, Piiceon PCMCIA 14.4 and 14.4 for Contura+LTE (ISA)
AddReg=All, MfgAddReg, Rockwell29.AddReg, INTERNAL

[Rockwell34] ; Piiceon 14.4 for toshiba
AddReg=All, MfgAddReg, Rockwell34.AddReg, INTERNAL

[Rockwell35] ; Cardinal+CPI (Viva) V.34
AddReg=All, MfgAddReg, Rockwell35.AddReg, EXTERNAL

[Rockwell36] ; Cardinal 14.4 mvp144xf
AddReg=All, MfgAddReg, Rockwell10.AddReg, EXTERNAL

[Rockwell37] ; Cardinal 14.4 data fax mvp144e
AddReg=All, MfgAddReg, Rockwell37.AddReg, EXTERNAL

[Rockwell38] ; Cardinal 28.8 V.34-VFC internal
AddReg=All, MfgAddReg, Rockwell35.AddReg, INTERNAL

[Rockwell39] ; Cardinal 14.4 Data FAX MVP144IF
AddReg=All, MfgAddReg, Rockwell37.AddReg, INTERNAL

[Rockwell40] ; Piiceon V.34 PCMCIA
AddReg=All, MfgAddReg, Rockwell40.AddReg, PCMCIA

[Rockwell41] ; Piiceon, Smart, other PCMCIA (disable inactivity timer)
AddReg=All, MfgAddReg, Rockwell41.AddReg, PCMCIA

[Rockwell42] ; Cardinal 19.2 data fax MVP192I
AddReg=All, MfgAddReg, Rockwell42.AddReg, INTERNAL

[Rockwell43] ; Winbook internal modem
AddReg=All, MfgAddReg, Rockwell27.AddReg, INTERNAL

[Rockwell44] ; Reveal 14.4 Modem Soundcard
AddReg=All, MfgAddReg, Rockwell44.AddReg, INTERNAL

; AddReg sections

[Rockwell1.AddReg] ; (internal 14400)
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00

[Rockwell2.AddReg] ; (internal 14400)
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"

[Rockwell3.AddReg] ; (external 14400) - Best Data
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell4.AddReg] ; (internal 14400) - Best Data
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell5.AddReg] ; (internal 28.8) - Best Data
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell6.AddReg] ; (internal 28.8) - Best Data and Zoom combo
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell9.AddReg] ; (external 14400) - Best Data 1442FX (FTX, RPI model)
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f0,03,00,00, 00,e1,00,00, 40,38,00,00
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell10.AddReg] ; (internal 14400) - Best Data 1442FX (FT, RPI model)
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f0,03,00,00, 00,c2,01,00, 40,38,00,00
HKR,, InactivityScale, 1, 0a,00,00,00

[Rockwell11.AddReg] ; (internal 2400) - Best Data 9624FQ 
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, 40,03,00,00, 60,09,00,00, 60,09,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 S0=0<cr>"
HKR, Settings, DialSuffix,, ""

[Rockwell12.AddReg] ; (external 2400) - Best Data 9648Fx, 2400B, 2400X and other modems
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, 40,03,00,00, 60,09,00,00, 60,09,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 S0=0<cr>"
HKR, Settings, DialSuffix,, ""

[Rockwell13.AddReg] ; Smart V.34 PCMCIA
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 0a,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell14.AddReg] ; SMART ST1414 PCMCIA with cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 0a,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell15.AddReg] ; Apex V.34 PCMCIA and Tosh combo. 
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N7 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N6 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C1"    
HKR, Settings, ErrorControl_On,, "\N7"
HKR, Settings, ErrorControl_Forced,, "\N6"

[Rockwell16.AddReg] ; PCMCIA 2400 bps, 19.2 max dte, no cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,4b,00,00, 60,09,00,00
HKR,, InactivityScale, 1, 01,00,00,00
HKR, Init, 2,, "AT&FE0V1&D2&C1S95=47S0=0&C1&D2<cr>"
HKR, Settings, Compression_On,, "%%C3"

[Rockwell17.AddReg] ; Com1 by AT&T (Keep in Touch PCMCIA)
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 07,00,00,00, 77,03,00,00, 00,e1,00,00, 40,38,00,00
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init, 2,, "AT &F S0=0 &D2 E0 V1<cr>"
HKR, Settings, DialSuffix,, ""
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,, "\N7"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N6"
HKR, Settings, InactivityTimeout,, "\T<#>"

[Rockwell18.AddReg]  ; (internal 14400) - no speed negotiation, inactivity timer is \Tn with max 90 minutes
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, 77,03,00,00, 00,e1,00,00, 40,38,00,00
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, InactivityTimeout,, "\T<#>"

[Rockwell21.AddReg] ; (internal 14400) - with cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"

[Rockwell22.AddReg]  ; (external 14400) - Logicode data-fax-voice with cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"

[Rockwell23.AddReg] ; (external 14400)  Logicode and Microcom combo
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, c3,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"

[Rockwell24.AddReg] ; (internal 14400) - cirrus chipset found in Logicode, no cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 \V2 S0=0<cr>"
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,,"\N3-J1"          
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N4-J1"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, InactivityTimeout,, "\T<#>"

[Rockwell25.AddReg] ; (internal 2400) - Logicode 9426
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 60,09,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 S0=0 S95=47<cr>"
HKR, Settings, Compression_On,, "%%C3"
HKR,, InactivityScale, 1, 0a,00,00,00    ; 10 sec

[Rockwell27.AddReg] ; (PCMCIA 14400, no cell, cirrus chipset) - Logicode
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 \V2 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, InactivityTimeout,, "\T<#>"
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,,"\N3-J1"          
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N4-J1"

[Rockwell28.AddReg] ; (internal 1200)  - no compr, ec, speed neg, hard flow, cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, 40,03,00,00, b0,04,00,00, b0,04,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 S0=0<cr>"

[Rockwell29.AddReg] ; Piiceon Dispatcher 14.4 with cell
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W1 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"                                                

[Rockwell30.AddReg] ; Piiceon Dispatcher V.34
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell31.AddReg] ; Winbook 14.4 Internal
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 \V2 S0=0<cr>"
HKR,, InactivityScale, 1, 01,00,00,00
HKR, Settings, InactivityTimeout,, "\T<#>"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,,"\N3-J1"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N4-J1"
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"

[Rockwell32.AddReg] ; Logicode ISA and Viva 14.4 PCMCIA 
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f3,03,00,00, 00,e1,00,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 \V2 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,,"\N3"          
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, InactivityTimeout,, "\T<#>"

[Rockwell34.AddReg] ; Piiceon Dispatcher 14.4 with cell for Toshiba
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 *H1"
HKR, Settings, Compression_On,, "%%C3"                                                

[Rockwell35.AddReg] ; cardinal, CPI V.34 combo
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell37.AddReg] ; Cardinal 14.4 data fax mvp144e
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,e1,00,00, 40,38,00,00
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1\V1W2S95=47S0=0<cr>"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, ErrorControl_Forced,, "\N4"
HKR, Settings, Modulation_CCITT,, "B0B15"
HKR, Settings, Modulation_Bell,, "B1B16"
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"

[Rockwell40.AddReg] ; Piiceon V.34 PCMCIA
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell41.AddReg] ; Smart, Piiceon PCMCIA, disable inactivity timer
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, ff,03,00,00, 00,c2,01,00, 80,70,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 W2 S95=47 S0=0<cr>"
HKR, Settings, ErrorControl_Cellular,, "\N3 -K1 )M1 -Q1 *H1"
HKR, Settings, ErrorControl_Cellular_Forced,, "\N2 -K1 )M1 -Q1 *H1"
HKR, Settings, Compression_On,, "%%C3"    

[Rockwell42.AddReg] ; Cardinal 19.2 internal, MVP192I
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 00,4b,00,00
HKR, Init, 2,, "AT&FE0V1&D2&C1\V1W2S95=47S0=0<cr>"
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, ErrorControl_Forced,, "\N4"
HKR, Settings, Modulation_CCITT,, "B0B15"
HKR, Settings, Modulation_Bell,, "B1B16"
HKR, Settings, Compression_On,, "%%C1""H3"
HKR, Settings, Compression_Off,, "%%C0""H0"

[Rockwell44.AddReg] ; Reveal 14.4 Modem Soundcard
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 40,38,00,00
HKR,, InactivityScale, 1, 0a,00,00,00 
HKR, Settings, Compression_On,, "%%C3"

; Strings

[Strings]

Reveal      = "Reveal"
Reveal1     = "Reveal 28.8, V.34, Data Fax PM700"
Reveal2     = "Reveal 14.4, Data Fax PM500"
Reveal4     = "Reveal Decathlon XL 14.4 Modem+Sound Card" 
Reveal5     = "14.4 Data Fax Voice Modem+Soundcard"

Winbook     = "Winbook"
Winbook1    = "Winbook (Dynalink) 14.4 Data Fax"
Winbook2    = "Winbook (Cirrus) 14.4 Data Fax"

Mitsubishi  = "Mitsubishi"
Mitsubishi1 = "Mitsubishi 14.4 PCMCIA"

Piiceon  = "Piiceon"
Piiceon2 = "Piiceon Dispatcher 14.4 PCMCIA"
Piiceon3 = "Piiceon Dispatcher V.34 for LTE and Contura"
Piiceon4 = "Piiceon Dispatcher 14.4 for LTE and Contura"
Piiceon5 = "Piiceon Dispatcher Modem"
Piiceon6 = "Piiceon Dispatcher 14.4 for Toshiba"    
Piiceon7 = "Piiceon Dispatcher 28.8, V.34 PCMCIA"    
Piiceon8 = "Piiceon Dispatcher PCMCIA"    

Macronix  = "Macronix"
Macronix1 = "Macronix 14.4 Data Fax PCMCIA"
Macronix2 = "Macronix 1200 bps Modem"

Premax  = "Premax"
Premax1 = "Premax 28.8, V.34 PCMCIA"
Premax2 = "Premax 28.8, VFC PCMCIA"
Premax3 = "28.8, V.34 PCMCIA Modem"     ; combo, premax and Smart Modular

Logicode  = "Logicode"
Logicode1 = "Logicode 28.8, V.34 External"             ; Logicode 28.8 V.34 External with cell
Logicode2 = "Logicode 28.8, V.34 Internal"             ; Logicode 28.8 V.34 Internal with cell
Logicode3 = "Logicode 14.4 Data-Fax-Voice Internal"    ; Logicode 14.4 Internal data-fax-voice with cell
Logicode4 = "Logicode 14.4 Data-Fax-Voice External"    ; Logicode 14.4 External data-fax-voice with cell
Logicode5 = "14.4 Data-Fax Modem"                      ; Logicode and Microcom combo
Logicode6 = "Logicode 14.4 Data-Fax External"          ; Logicode 14.4 Data-Fax External (No voice!)
Logicode7 = "Logicode 14.4 Data-Fax Internal 1414HV"   ; Logicode 14.4 Data-Fax External (No voice!)
Logicode8 = "Logicode 9624 Data-Fax Internal"          ; Logicode 9624 Data-Fax Internal
Logicode9 = "Logicode 9624 Data-Fax External"          ; Logicode 9624 Data-Fax External
Logicode13= "Logicode 14.4 Data Fax (RPI)"

Rockwell  ="Rockwell"
Rockwell1 ="14400 bps Data-Fax Modem"
Rockwell2 ="14400 bps Internal Data-Fax Modem"
Rockwell3 ="14400 bps Internal Data-Fax Modem"

Cardinal  ="Cardinal"
Cardinal1 ="Cardinal 14.4 Kbps Internal Fax Modem"
Cardinal2 ="Cardinal MVP288XF 28.8 Kbps V.34 Fax Modem"
Cardinal3 ="28.8, V.34-VFC Data Fax Modem"    ; Cardinal, CPI (Viva)
Cardinal4 ="Cardinal MVP144XF 14.4 Kbps Fax Modem"    
Cardinal5 ="Cardinal MVP144E 14.4 Kbps Fax Modem"    
Cardinal6 ="Cardinal MVP24XF 2400 Fax Modem"    
Cardinal7 ="Cardinal MVP144CC 14.4 Kbps PC Card"    
Cardinal8 ="Cardinal MVP288I 28.8 Kbps V.34 Fax Modem"    
Cardinal9 ="28.8, V.34-VFC Data Fax Modem"    ; Cardinal, CPI (Viva)
Cardinal10 ="Cardinal MVP144IF 14.4 Kbps Fax Modem"    
Cardinal11 ="Cardinal 14.4 Data Fax Modem"    ; MVP144IF, MVP144E
Cardinal12 ="Cardinal MVP144I 14.4 Kbps Fax Modem"
Cardinal13 ="Cardinal MB2650SR 2400 bps Fax Modem"
Cardinal14 ="Cardinal MVP192I 19.2 Fax Modem"

Digitan   ="Digitan"
Digitan2  ="Digitan 14400 bps Internal Data-Fax Modem"
Digitan3  ="Digitan 28.8, V.34 Data-Fax-Voice Modem"
Digitan4  ="Digitan 28.8, V.34 Data-Fax-Modem"

BestData  = "Best Data"
BestData1 = "Best Data Smart One 1442FX Modem"       ; 1442FX External
BestData2 = "Best Data Smart One 1442F Modem"        ; 1442F Internal
BestData3 = "Best Data Smart One 2834F Modem"        ; 2834F Internal
BestData4 = "28.8 Internal modem"                    ; Zoom and Best data combo, INTERNAL
BestData5 = "Best Data Smart One 2834FX Modem"       ; Best Data 2834FX External 
BestData6 = "28.8 External modem"                    ; Zoom and Best data combo, EXTERNAL
BestData7 = "Best Data Smart One 1442FX (FTX, RPI)"  ; Best Data 1442FX External (FTX, RPI model)
BestData8 = "Best Data Smart One 1442F (FT, RPI)"    ; Best Data 1442FX Internal (FTX, RPI model)
BestData9 = "Best Data Smart One 9624FQ Modem"       ; Best Data 9624FQ internal
BestData10 = "Best Data Smart One 2400B Modem"       ; Best Data Smart One 2400B internal
BestData11 = "Best Data Smart One 9648FX Modem"      ; Best Data Smart One 9648FX external
BestData12 = "2400 bps Modem"                        ; Best Data Smart One 9648FX external and Viva combo
BestData13 = "Best Data Smart One 2400X Modem"       ; Best Data Smart One 2400X

SMART = "Smart Modular Technologies"
SmartMod1 ="SMART Modular Tech ST 1414 Cell PCMCIA"
SmartMod2 ="SMART Modular Tech ST 2814 V.34 PCMCIA"

Apex  = "Apex Data Inc."
Apex3 = "Apex V.34 Cellular PCMCIA Modem"
Apex4 = "V.34 Cellular PCMCIA Modem"   ; Apex and Toshiba combo

ComOne = "Com 1"
ComOne6="COM1-SA MC218 V.34 PCMCIA"        ; MC218 28.8 data fax voice
ComOne4="COM1-SA MC216 14.4 PCMCIA"        ; MC216 
ComOne2="COM1-SA MC214 2400 PCMCIA"        ; MC214A
ComOne1="COM1-SA MC217 14.4 PCMCIA"        ; MC217A 14.4 data fax voice
; ComOne13="PCMCIA S214 V22bis Fax-Modem"
; ComOne12="PCMCIA SLIMFAXII Fax-Modem"
; ComOne11="PCMCIA S218 V34 Fax-Modem"
; ComOne10="PCMCIA SLIMV34 Fax-Modem"
; ComOne9="PCMCIA S217 V32bis Fax-Modem"
; ComOne8="PCMCIA AJ 1448 V32bis Fax-Modem"
; ComOne7="PCMCIA SLIM144 Fax-Modem"
; ComOne5="COM1-SA MV216 COM1-SA V32bis Data-Fax PCMCIA"
; ComOne3="COM1-SA MV129 V22bis Data-Fax PCMCIA"

[All]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init, 1,, "AT<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00

[EXTERNAL]
HKR,, DeviceType, 1, 01

[INTERNAL]
HKR,, DeviceType, 1, 02

[PCMCIA]
HKR,,PortDriver,,serial.vxd
HKR,,Contention,,*vcd
HKR,, DeviceType, 1, 03

[MfgAddReg]
HKR,, InactivityScale, 1, 01,00,00,00
HKR, Init, 2,, "AT &F E0 V1 &D2 &C1 S95=47 W1 S0=0<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Hangup, 1,, "ATH<cr>"
HKR, Answer, 1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ";"
HKR, Settings, SpeakerVolume_Low,, "L0"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "&K0"
HKR, Settings, FlowControl_Hard,, "&K3"
HKR, Settings, FlowControl_Soft,, "&K4"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N2"
HKR, Settings, Compression_On,, "%%C1"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Modulation_CCITT,, "B0"
HKR, Settings, Modulation_Bell,, "B1"
HKR, Settings, SpeedNegotiation_Off,, "N0"
HKR, Settings, SpeedNegotiation_On,, "N1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "S30=<#>"

HKR, Responses, "<cr>",        1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<lf>",        1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
HKR, Responses, "OK",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "RING",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NO CARRIER",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "ERROR",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NO DIALTONE", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NO DIAL TONE",1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "BUSY",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NO ANSWER",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "FAX",         1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DATA",        1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "VOICE",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "RINGING",     1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DELAYED",     1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "BLACKLISTED", 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "+FCERROR",    1, 03, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "CONNECT",                 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/ARQ",             1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/REL",             1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/MNP",             1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/LAP-M",           1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/V42BIS",          1, 02, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT/V42b",            1, 02, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300",             1, 02, 00, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/ARQ",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/REL",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/REL-MNP",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/REL-MNP 5",         1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/REL-LAPM",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/REL-LAPM V.42 BIS",         1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/MNP",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/LAP-M",       1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/V42BIS",      1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 300/V42b",        1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600",             1, 02, 00, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/ARQ",         1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/REL",         1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/REL-MNP",           1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/REL-MNP 5",         1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/REL-LAPM",          1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/REL-LAPM V.42 BIS", 1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/MNP",         1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/LAP-M",       1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/V42BIS",      1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 600/V42b",        1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600",            1, 02, 00, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/ARQ",        1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/REL",        1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/MNP",        1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/LAP-M",      1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/V42BIS",     1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 0600/V42b",       1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200",            1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/ARQ",        1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/REL",        1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/REL-MNP",           1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/REL-MNP 5",         1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/REL-LAPM",          1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/REL-LAPM V.42 BIS", 1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/MNP",        1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/LAP-M",      1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/V42BIS",     1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/V42b",       1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75",         1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/ARQ",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/REL",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/MNP",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/LAP-M",   1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/V42BIS",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200/75/V42b",    1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX",     1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/ARQ", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/REL", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/MNP", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/LAP-M", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/V42BIS",1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 1200TX/75RX/V42b",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200",         1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/ARQ",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/REL",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/MNP",     1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/LAP-M",   1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/V42BIS",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75/1200/V42b",    1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX",     1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/ARQ", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/REL", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/MNP", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/LAP-M", 1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/V42BIS",1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 75TX/1200RX/V42b",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400",            1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/ARQ",        1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/REL",        1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/REL-MNP",           1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/REL-MNP 5",         1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/REL-LAPM",          1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/REL-LAPM V.42 BIS", 1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/MNP",        1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/LAP-M",      1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/V42BIS",     1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 2400/V42b",       1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800",            1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/ARQ",        1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/REL",        1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/REL-MNP",           1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/REL-MNP 5",         1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/REL-LAPM",          1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/REL-LAPM V.42 BIS", 1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/MNP",        1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/LAP-M",      1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/V42BIS",     1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 4800/V42b",       1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200",            1, 02, 00, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/ARQ",        1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/REL",        1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/REL-MNP",           1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/REL-MNP 5",         1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/REL-LAPM",          1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/REL-LAPM V.42 BIS", 1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/MNP",        1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/LAP-M",      1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/V42BIS",     1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 7200/V42b",       1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600",            1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/ARQ",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/REL",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/REL-MNP",           1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/REL-MNP 5",         1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/REL-LAPM",          1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/REL-LAPM V.42 BIS", 1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/MNP",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/LAP-M",      1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/V42BIS",     1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 9600/V42b",       1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000",           1, 02, 00, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/ARQ",       1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/REL",       1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/REL-MNP",           1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/REL-MNP 5",         1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/REL-LAPM",          1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/REL-LAPM V.42 BIS", 1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/MNP",       1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/LAP-M",     1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/V42BIS",    1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 12000/V42b",      1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400",           1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/ARQ",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/REL",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/REL-MNP",           1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/REL-MNP 5",         1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/REL-LAPM",          1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/REL-LAPM V.42 BIS", 1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/MNP",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/LAP-M",     1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/V42BIS",    1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 14400/V42b",      1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800",           1, 02, 00, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/ARQ",       1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/REL",       1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/MNP",       1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/LAP-M",     1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/V42BIS",    1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 16800/V42b",      1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200",           1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/ARQ",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/REL",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/MNP",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/LAP-M",     1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/V42BIS",    1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 19200/V42b",      1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "CONNECT 21600",           1, 02, 00, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/ARQ",       1, 02, 02, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/REL",       1, 02, 02, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/MNP",       1, 02, 02, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/LAP-M",     1, 02, 02, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/V42BIS",    1, 02, 03, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 21600/V42b",      1, 02, 03, 60,54,00,00, 00,00,00,00 
HKR, Responses, "CONNECT 24000",           1, 02, 00, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/ARQ",       1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/REL",       1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/MNP",       1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/LAP-M",     1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/V42BIS",    1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 24000/V42b",      1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400",           1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/ARQ",       1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/REL",       1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/MNP",       1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/LAP-M",     1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/V42BIS",    1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 26400/V42b",      1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800",           1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/ARQ",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/REL",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/MNP",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/LAP-M",     1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/V42BIS",    1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 28800/V42b",      1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400",           1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/ARQ",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/REL",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/MNP",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/LAP-M",     1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/V42BIS",    1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 38400/V42b",      1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600",           1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/ARQ",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/REL",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/MNP",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/LAP-M",     1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/V42BIS",    1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 57600/V42b",      1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "CONNECT 115200",          1, 02, 00, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/ARQ",      1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/REL",      1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/MNP",      1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/LAP-M",    1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/V42BIS",   1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115200/V42b",     1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200",         1, 02, 00, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/ARQ",     1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/REL",     1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/MNP",     1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/LAP-M",   1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/V42BIS",  1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "CONNECT 115,200/V42b",    1, 02, 03, 00,C2,01,00, 00,00,00,00

HKR, Responses, "CARRIER 300",       1, 01, 00, 2c,01,00,00, 00,00,00,00
HKR, Responses, "CARRIER 1200",      1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 1200/75",   1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 75/1200",   1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 2400",      1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "CARRIER 4800",      1, 01, 00, c0,12,00,00, 00,00,00,00
HKR, Responses, "CARRIER 7200",      1, 01, 00, 20,1c,00,00, 00,00,00,00
HKR, Responses, "CARRIER 9600",      1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "CARRIER 12000",     1, 01, 00, e0,2e,00,00, 00,00,00,00
HKR, Responses, "CARRIER 14400",     1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "CARRIER 16800",     1, 01, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "CARRIER 19200",     1, 01, 00, 00,4b,00,00, 00,00,00,00
HKR, Responses, "CARRIER 21600",     1, 01, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "CARRIER 24000",     1, 01, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "CARRIER 26400",     1, 01, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "CARRIER 28800",     1, 01, 00, 80,70,00,00, 00,00,00,00

HKR, Responses, "CARRIER 300/VFC",       1, 01, 00, 2c,01,00,00, 00,00,00,00
HKR, Responses, "CARRIER 1200/VFC",      1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 1200/75/VFC",   1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 75/1200/VFC",   1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "CARRIER 2400/VFC",      1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "CARRIER 4800/VFC",      1, 01, 00, c0,12,00,00, 00,00,00,00
HKR, Responses, "CARRIER 7200/VFC",      1, 01, 00, 20,1c,00,00, 00,00,00,00
HKR, Responses, "CARRIER 9600/VFC",      1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "CARRIER 12000/VFC",     1, 01, 00, e0,2e,00,00, 00,00,00,00
HKR, Responses, "CARRIER 14400/VFC",     1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "CARRIER 16800/VFC",     1, 01, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "CARRIER 19200/VFC",     1, 01, 00, 00,4b,00,00, 00,00,00,00
HKR, Responses, "CARRIER 21600/VFC",     1, 01, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "CARRIER 24000/VFC",     1, 01, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "CARRIER 26400/VFC",     1, 01, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "CARRIER 28800/VFC",     1, 01, 00, 80,70,00,00, 00,00,00,00

HKR, Responses, "COMPRESSION: CLASS5",   1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: CLASS 5",  1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: MNP5",     1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: V42BIS",   1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: V.42BIS",  1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: V.42 BIS", 1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: V.42bis",  1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: V.42 bis", 1, 01, 03, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: ADC",      1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "COMPRESSION: NONE",     1, 01, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "PROTOCOL: NONE",                   1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: LAPM",                   1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: LAP-M",                  1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: ALT",                    1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: MNP",                    1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: MNP2",                   1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: MNP3",                   1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "PROTOCOL: MNP4",                   1, 01, 02, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 300/V42<cr><lf>",     1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/V42<cr><lf>",    1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/V42<cr><lf>",    1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/V42<cr><lf>",    1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/V42<cr><lf>",    1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/V42<cr><lf>",    1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/V42<cr><lf>",   1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/V42<cr><lf>",   1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/V42<cr><lf>",   1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/V42<cr><lf>",   1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/V42<cr><lf>",   1, 02, 02, 60,54,00,00, 00,00,00,00 
HKR, Responses, "<cr><lf>CONNECT 24000/V42<cr><lf>",   1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/V42<cr><lf>",   1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/V42<cr><lf>",   1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/V42<cr><lf>",   1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/V42<cr><lf>",   1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/V42<cr><lf>",  1, 02, 02, 00,C2,01,00, 00,00,00,00
