; Copyright (c) 1993-1995 Microsoft Corporation

[version]
signature="$CHICAGO$"
Class=hdc
Provider=%MS%

;Class Install
[ClassInstall]
AddReg=HDC_Class

[HDC_Class]
HKR,,,,%HDCClassName%
HKR,,Icon,,-9

[Manufacturer]
%MS-Drivers%=MS_HDC
%ALI%=ALI_HDC
%APPIAN%=APPIAN_HDC
%CMD%=CMD_HDC
%COMPAQ%=COMPAQ_HDC
%DATATECH%=DATATECH_HDC
%INTEGRAL%=Integral_HDC
%KINGSTON%=KINGSTON_HDC
%IBM%=IBM_HDC
%INTEL%=INTEL_HDC
%MAXTOR%=MAXTOR_HDC
%MINISTOR%=MINISTOR_HDC
%NATSEMI%=NATSEMI_HDC
%OPTI%=OPTI_HDC
%PCTECH%=PCTECH_HDC
%SD%=SD_HDC
%SYMPHONY%=SYMPHONY_HDC
%VIATECH%=VIATECH_HDC
%ZENITH%=ZENITH_HDC
%CREATIVELABS%=CREATIVELAB_HDC

[MS_HDC]
%*pnp0601.DeviceDesc%   = HardCardII, *PNP0601     ;Plus_Hardcard_II
%*PNP0602.DeviceDesc%   = HardCardIIXL, *PNP0602   ;Plus_Hardcard_IIXL/EZ
%*PNP0600.DeviceDesc%   = BAD_IDE, *PNP0600        ;Generic_ESDI_Hard_Disk_Controller
%*PNP0603.DeviceDesc%   = GOOD_IDE, *PNP0603       ;Generic_ESDI_Hard_Disk_Controller
%*ZDS2010.DeviceDesc%   = GOOD_IDE, *ZDS2010       ;Zeos EISA IDE
%PCI\CC_0101.DeviceDesc%= UNKNOWN_PCI_IDE, PCI\CC_0101;Generic PCI IDE
%MF\BADPRIMARY.DeviceDesc% = BAD_IDE, MF\BADPRIMARY
%MF\BADSECONDARY.DeviceDesc% = BAD_IDE, MF\BADSECONDARY
%MF\GOODPRIMARY.DeviceDesc% = GOOD_IDE, MF\GOODPRIMARY
%MF\GOODSECONDARY.DeviceDesc% = GOOD_IDE, MF\GOODSECONDARY

[ALI_HDC]
%PCI\VEN_10B9&DEV_5215.DeviceDesc%=UNKNOWN_PCI_IDE, PCI\VEN_10B9&DEV_5215

[APPIAN_HDC]
%PCI\VEN_1097&DEV_0038.DeviceDesc%=BAD_IDE, PCI\VEN_1097&DEV_0038

[CMD_HDC]
%PCI\VEN_1095&DEV_0640.DeviceDesc%=DUAL_BAD_IDE, PCI\VEN_1095&DEV_0640
%PCI\VEN_1095&DEV_0646.DeviceDesc%=DUAL_BAD_IDE, PCI\VEN_1095&DEV_0646

[COMPAQ_HDC]
%*CPQA0DA.DeviceDesc%   = GOOD_IDE, *CPQA0DA       ;Compaq IDE
%*CPQ4300.DeviceDesc%   = GOOD_IDE, *CPQ4300       ;Compaq EISA Advanced ESDI

[DATATECH_HDC]
%PCI\VEN_1C1C&DEV_0001.DeviceDesc%=GOOD_IDE, PCI\VEN_1C1C&DEV_0001

[KINGSTON_HDC]
%PCMCIA\KINGSTON_TECHNOLOGY-DATAPAK_170-3B77.DeviceDesc%=GOOD_IDE, PCMCIA\KINGSTON_TECHNOLOGY-DATAPAK_170-3B77

[IBM_HDC]
%mca_df9f.DeviceDesc%	= IBMIDE,mca_df9f	;IBM Integrated Fixed Disk

[INTEL_HDC]
%PCI\VEN_8086&DEV_1222.DeviceDesc%=DUAL_GOOD_IDE, PCI\VEN_8086&DEV_1222
%PCI\VEN_8086&DEV_1230.DeviceDesc%=DUAL_GOOD_IDE, , PCI\VEN_8086&DEV_1230

[Integral_HDC]
%Integral.DeviceDesc%=GOOD_IDE, PCMCIA\INTEGRAL_PERIPHERALS-ATA_CARD-456B

[MAXTOR_HDC]
%PCMCIA\MAXTOR-MXL105-E950.DeviceDesc%=MAXTOR_drv, PCMCIA\MAXTOR-MXL105-E950
%PCMCIA\MAXTOR-MXL105-352F.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL105-352F
%PCMCIA\MAXTOR-MXL131.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL131-351E
%PCMCIA\MAXTOR-MXL131.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL131-84AD
%PCMCIA\MAXTOR-MXL131.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL131-BA9C
%PCMCIA\MAXTOR-MXL171.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL171-764B
%PCMCIA\MAXTOR-MXL262.DeviceDesc%=GOOD_IDE, PCMCIA\MAXTOR-MXL262-13BA

[MINISTOR_HDC]
%PCMCIA\MINISTOR-MP130P-FEED.DeviceDesc%=GOOD_IDE, PCMCIA\MINISTOR-MP130P-FEED
%Ministor170.DeviceDesc%=GOOD_IDE, PCMCIA\MINISTOR-MP170P-CF02

[NATSEMI_HDC]
%PCI\VEN_100B&DEV_D001.DeviceDesc%=DUAL_BAD_IDE, PCI\VEN_100B&DEV_D001

[OPTI_HDC]
%PCI\VEN_1045&DEV_C621.DeviceDesc%=DUAL_BAD_IDE, PCI\VEN_1045&DEV_C621

[PCTECH_HDC]
%PCI\VEN_1042&DEV_1000.DeviceDesc%=UNKNOWN_PCI_IDE, PCI\VEN_1042&DEV_1000

[SD_HDC]
%PCMCIA\SunDisk-SDP.DeviceDesc%=SUNDISK_drv, PCMCIA\SunDisk-SDP-1E2E
%PCMCIA\SunDisk-SDP.DeviceDesc%=SUNDISK_drv, PCMCIA\SunDisk-SDP-1DD2
%PCMCIA\SunDisk-SDP.DeviceDesc%=SUNDISK_drv, PCMCIA\SunDisk-SDP5-ADFD
%PCMCIA\SunDisk-SDP.DeviceDesc%=SUNDISK_drv, PCMCIA\SunDisk-SDP-6DC7
%PCMCIA\SunDisk-SDP.DeviceDesc%=SUNDISK_drvl5, PCMCIA\SunDisk-SDPL5-F150

[SYMPHONY_HDC]
%PCI\VEN_10AD&DEV_0001.DeviceDesc%=BAD_IDE, PCI\VEN_10AD&DEV_0001

[VIATECH_HDC]
%PCI\VEN_1106&DEV_0561.DeviceDesc%=DUAL_BAD_IDE, PCI\VEN_1106&DEV_0561

[ZENITH_HDC]
%MF\EISA_ZDS2000_DEV0.DeviceDesc%=GOOD_IDE, MF\EISA_ZDS2000_DEV0

[CREATIVELAB_HDC]
%*CTL2011.DeviceDesc%= GOOD_IDE, *CTL2011



[*pnp0601.det]          ;Plus Hardcard II
LogConfig=hclc1,hclc2
AddReg = HDC_HW_REG

[HardCardII]
LogConfig=hclc1,hclc2
AddReg = HARDCARD_AddReg

[hclc1]
ConfigPriority=HARDWIRED
IRQConfig=10,11,12
MEMConfig=C800-C80F,CC00-CC0F,D000-D00F,D400-D40F
IOConfig=170-177(3FF::)
IOConfig=376-377(3FF::)

[hclc2]
ConfigPriority=HARDWIRED
IRQConfig=10,11,12
MEMConfig=CA00-CA0F,CE00-CE0F,D200-D20F,D600-D60F
IOConfig=320-327(3FF::)
IOConfig=32E-32F(3FF::)

[*pnp0602.det]
LogConfig=hclc1,hclc2
AddReg = HDC_HW_REG

[HardCardIIXL]
LogConfig=hclc1,hclc2
AddReg = HARDCARD_AddReg

[*pnp0600.det]          ;ESDI Controller
LogConfig=esdilc1,esdilc2
AddReg = HDC_HW_REG

[esdilc1]
ConfigPriority=HARDWIRED
IOConfig=1f0-1f7(3ff::)
IOConfig=3f6-3f6(3ff::)
IRQConfig=S:14

[esdilc2]
ConfigPriority=HARDWIRED
IOConfig=170-177(3ff::)
IOConfig=376-376(3ff::)
IRQConfig=S:15

[BAD_IDE]
LogConfig=esdilc1,esdilc2
AddReg = ESDI_AddReg

[BAD_IDE.PosDup]
*PNP0600

[GOOD_IDE]
LogConfig=esdilc1,esdilc2
AddReg = ESDI_AddReg

[GOOD_IDE.HW]
AddReg = ESDI_FIFO_OK_AddReg

[GOOD_IDE.PosDup]
*PNP0600

[UNKNOWN_PCI_IDE]
AddReg=PCIMF.Reg

[UNKNOWN_PCI_IDE.HW]
AddReg=UNKNOWN_PCI_IDE.RegHW,DontStopChild.RegHW

[UNKNOWN_PCI_IDE.RegHW]
HKR,Child0000,HardwareID,,MF\BADPRIMARY
HKR,Child0000,ResourceMap,1,00,01,02
HKR,Child0000,MFFlags,1,08,00,00,00
HKR,Child0001,HardwareID,,MF\BADSECONDARY
HKR,Child0001,ResourceMap,1,03,04,05
HKR,Child0001,MFFlags,1,08,00,00,00

[UNKNOWN_PCI_IDE.PosDup]
*PNP0600

[DUAL_BAD_IDE]
AddReg=PCIMF.Reg

[DUAL_BAD_IDE.HW]
AddReg=DUAL_BAD_IDE.RegHW,DontStopChild.RegHW

[DUAL_BAD_IDE.RegHW]
HKR,Child0000,HardwareID,,MF\BADPRIMARY
HKR,Child0000,ResourceMap,1,00,01,02
HKR,Child0000,MFFlags,1,08,00,00,00
HKR,Child0001,HardwareID,,MF\BADSECONDARY
HKR,Child0001,ResourceMap,1,03,04,05
HKR,Child0001,MFFlags,1,08,00,00,00
HKR,,PCIDualIDE,1,01

[DUAL_BAD_IDE.PosDup]
*PNP0600

[DUAL_GOOD_IDE]
AddReg=PCIMF.Reg

[DUAL_GOOD_IDE.HW]
AddReg=DUAL_GOOD_IDE.RegHW

[DUAL_GOOD_IDE.RegHW]
HKR,Child0000,HardwareID,,MF\GOODPRIMARY
HKR,Child0000,ResourceMap,1,00,01,02
HKR,Child0000,MFFlags,1,08,00,00,00
HKR,Child0001,HardwareID,,MF\GOODSECONDARY
HKR,Child0001,ResourceMap,1,03,04,05
HKR,Child0001,MFFlags,1,08,00,00,00
HKR,,PCIDualIDE,1,01

[DUAL_GOOD_IDE.PosDup]
*PNP0600

[PCIMF.Reg]
HKR,,DevLoader,,*CONFIGMG
HKR,,Enumerator,,*CONFIGMG
HKR,,CMDrivFlags,1,03,00,00,00

[DontStopChild.RegHW]
HKR,,ConfigFlags,1,80,00,00,00

[MAXTOR_drv]
AddReg = ESDI_AddReg,MAXTOROVERRIDE

[MAXTOROVERRIDE]
HKR,Override,0000,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,00,00,00, \
;
; I/O
;
24,00,00,00, \
02,00,00,00, \
01,00,0C,00, \
00,00,00,00, \
00,00,00,00, \
F0,FF,10,00, \
00,00,FF,FF, \
00,00,00,00, \
40,00,00,00, \
;
; IRQ
;
14,00,00,00, \
04,00,00,00, \
00,00,00,00, \
FF,FF,00,00, \
20,00,00,00, \
;
; REQUEST_CONFIG_PKT
;
19,00,00,00, \
7C,89,00,00, \
00,00,02,00, \
32,00,00,02, \
00,02,00,00, \
00,00,00,01, \
0F, \
;
; TERMINATOR
;
00,00,00,00

[SUNDISK_drv]
AddReg = ESDI_AddReg,SUNDISK_ScanDisk

[SUNDISK_drv.HW]
AddReg = ESDI_FIFO_OK_AddReg

[SUNDISK_drvl5]
AddReg = ESDI_AddReg, SUNDISK_ScanDisk, SDL5_OVERRIDE

[SUNDISK_drvl5.HW]
AddReg = ESDI_FIFO_OK_AddReg

[SDL5_OVERRIDE]
HKR,Override,0000,1, \
;
00,04,00,00, \
00,00,00,00, \
;
; IO Resource Descriptor
;
24,00,00,00, \
02,00,00,00, \
01,00,0c,00, \
00,00,00,00, \
00,00,00,00, \
f0,ff,08,00, \
00,00,ff,ff, \
00,00,00,00, \
40,00,00,00, \
;
; NO Memory Resource Descriptor
;
; IRQ Resource Descriptor
;
14,00,00,00, \
04,00,00,00, \
00,00,00,00, \
ff,ff,00,00, \
20,00,00,00, \
;
;
;REQUEST_CONFIG_PKT Descriptor
;
;
;Request Config Packet for SDPL5 Mode 1
19,00,00,00, \
7C,89,00,00, \
00,00,02,00, \
32,00,00,02, \
00,02,00,00, \
00,00,00,41, \
0F, \
;
; Terminator
;
00,00,00,00

[HARDCARD_AddReg]
HKR,,No_Driver,,"Uses RMode Mapper"

[IBMIDE]
 
[ESDI_FIFO_OK_AddReg]
HKR,,IDENoSerialize,3,01

[ESDI_AddReg]
HKR,,DriverDesc,,"ESDI Port Driver"
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,ESDI_506.pdr

[SUNDISK_ScanDisk]
HKR,,ScanOnlyFirstDrive,1,1

[HDC_HW_REG]
HKR,,NoSetupUI,,1

[ControlFlags]
CopyFilesOnly=PCMCIA\KINGSTON_TECHNOLOGY-DATAPAK_170-3B77
CopyFilesOnly=PCMCIA\MAXTOR-MXL105-E950,PCMCIA\MAXTOR-MXL105-352F
CopyFilesOnly=PCMCIA\MAXTOR-MXL131-351E,PCMCIA\MAXTOR-MXL131-84AD
CopyFilesOnly=PCMCIA\MAXTOR-MXL131-BA9C,PCMCIA\MAXTOR-MXL262-13BA
CopyFilesOnly=PCMCIA\MAXTOR-MXL171-764B,PCMCIA\MINISTOR-MP130P-FEED
CopyFilesOnly=PCMCIA\SunDisk-SDP-1E2E,PCMCIA\SunDisk-SDP-1DD2
CopyFilesOnly=PCMCIA\SunDisk-SDP5-ADFD,PCMCIA\SunDisk-SDP-6DC7
CopyFilesOnly=PCMCIA\SunDisk-SDPL5-F150
CopyFilesOnly=*ZDS2010,*CPQA0DA,*CPQ4300
CopyFilesOnly=PCI\VEN_1095&DEV_0640,PCI\VEN_1C1C&DEV_0001
CopyFilesOnly=PCI\VEN_8086&DEV_1222,PCI\VEN_1042&DEV_1000
CopyFilesOnly=PCI\VEN_1097&DEV_0038
CopyFilesOnly=PCI\CC_0101
CopyFilesOnly=MF\EISA_ZDS2000_DEV0
CopyFilesOnly=PCI\VEN_10AD&DEV_0001,PCI\VEN_1106&DEV_0561
CopyFilesOnly=PCI\VEN_1045&DEV_C621
CopyFilesOnly=PCI\VEN_10B9&DEV_5215
CopyFilesOnly=PCI\VEN_8086&DEV_1230
ExcludeFromSelect=MF\BADPRIMARY,MF\BADSECONDARY,MF\GOODPRIMARY,MF\GOODSECONDARY
CopyFilesOnly=*CTL2011


[Strings]
HDCClassName            = "Hard disk controllers"
MS-Drivers= "(Standard hard disk drivers)"
*pnp0601.DeviceDesc     = "Plus Hardcard II"
*PNP0602.DeviceDesc     = "Plus Hardcard IIXL/EZ"
*PNP0600.DeviceDesc     = "Standard IDE/ESDI Hard Disk Controller"
*PNP0603.DeviceDesc     = "Standard IDE/ESDI Hard Disk Controller (no serialization)"
*ZDS2010.DeviceDesc	= "Zeos EISA IDE Controller"
PCI\CC_0101.DeviceDesc  = "Standard Dual PCI IDE Controller"
MF\BADPRIMARY.DeviceDesc= "Primary IDE controller (single fifo)"
MF\BADSECONDARY.DeviceDesc= "Secondary IDE controller (single fifo)"
MF\GOODPRIMARY.DeviceDesc= "Primary IDE controller (dual fifo)"
MF\GOODSECONDARY.DeviceDesc= "Secondary IDE controller (dual fifo)"
ALI="Acer Labs Inc"
PCI\VEN_10B9&DEV_5215.DeviceDesc="ALI PCI IDE Controller"
APPIAN="Appian Technology"
PCI\VEN_1097&DEV_0038.DeviceDesc="Appian PCI IDE Controller"
CMD="CMD Technology"
PCI\VEN_1095&DEV_0640.DeviceDesc="CMD PCI-0640 PCI to IDE Controller"
PCI\VEN_1095&DEV_0646.DeviceDesc="CMD PCI-0646 Bus Master PCI to IDE Controller"
COMPAQ="Compaq"
*CPQA0DA.DeviceDesc	= "Compaq IDE Controller"
*CPQ4300.DeviceDesc	= "Compaq Advanced ESDI Controller"
DATATECH="DTC Data Technology"
PCI\VEN_1C1C&DEV_0001.DeviceDesc="DTC 2130S PCI Bus to IDE Single Port Controller"
KINGSTON="Kingston Technology"
PCMCIA\KINGSTON_TECHNOLOGY-DATAPAK_170-3B77.DeviceDesc="Kingston Technology 170MB PCMCIA Hard Disk"
IBM="IBM"
mca_df9f.DeviceDesc="IBM MCA Integrated Fixed Disk and Controller"
INTEL="Intel"
PCI\VEN_8086&DEV_1222.DeviceDesc="Intel 82092AA PCI IDE Controller"
PCI\VEN_8086&DEV_1230.DeviceDesc="Intel PIIX PCI IDE Controller [Bus Mastering not supported]"
Integral="Integral Peripherals"
Integral.DeviceDesc="Integral Peripherals PCMCIA Hard Disk"
MAXTOR="Maxtor"
PCMCIA\MAXTOR-MXL105-E950.DeviceDesc="MobileMax 105MB PCMCIA Hard Disk (1U3B)"
PCMCIA\MAXTOR-MXL105-352F.DeviceDesc="MobileMax 105MB PCMCIA Hard Disk"
PCMCIA\MAXTOR-MXL131.DeviceDesc="MobileMax 131MB PCMCIA Hard Disk"
PCMCIA\MAXTOR-MXL171.DeviceDesc="MobileMax 171MB PCMCIA Hard Disk"
PCMCIA\MAXTOR-MXL262.DeviceDesc="MobileMax 262MB PCMCIA Hard Disk"
MINISTOR="MiniStor"
PCMCIA\MINISTOR-MP130P-FEED.DeviceDesc="MiniStor 131MB PCMCIA Hard Disk"
MiniStor170.DeviceDesc="MiniStor 170MB PCMCIA Hard Disk"
NATSEMI="National Semiconductor"
PCI\VEN_100B&DEV_D001.DeviceDesc="National Semiconductor Dual PCI IDE Controller (RMM Support Only)"
OPTI="Opti"
PCI\VEN_1045&DEV_C621.DeviceDesc="Opti Dual PCI IDE Controller"
PCTECH="PC Technology"
PCI\VEN_1042&DEV_1000.DeviceDesc="PC Tech PCI IDE Single or Dual Port Controller"
SD="SunDisk"
PCMCIA\SunDisk-SDP.DeviceDesc="SunDisk ATA FlashDisk"
SYMPHONY="Symphony Labs"
PCI\VEN_10AD&DEV_0001.DeviceDesc="Symphony PCI IDE Controller"
VIATECH="VIA Tech"
PCI\VEN_1106&DEV_0561.DeviceDesc="VIA Tech Dual PCI IDE Controller"
Zenith="Zenith Data Systems"
MF\EISA_ZDS2000_DEV0.DeviceDesc="Standard IDE Controller on Zenith EISA board"
CREATIVELABS="Creative Labs"
*CTL2011.DeviceDesc="Creative Labs IDE controller"
